**TROŠKOVNIK**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| A | B | C |  | D | E=CxD |
| **Rd.br.** | **Specifikacija tražene opreme** | **Količina** | **Specifikacija ponuđene opreme (proizvođač, model, serija)** | **Jedinična cijena****(bez PDV-a)** | **Cijena****(bez PDV-a)** |
| 1. | CPU Desktop Core i7-14700K (up to 5.60 GHz, 33MB, LGA1700) box ili bolje | 11 |  |  |  |
| 2. | Hladnjak kompatibilan navedenoj CPU. Minimum 180W TDP | 11 |  |  |  |
| 3. | MB B760 LGA1700 - 4x DDR5 7200MHz (OC), 1 PCIe 5.0 x16, 1 PCIe 4.0 x16, 1 PCIe 3.0 x16, 1 PCIe 3.0 x1, Full ATX | 11 |  |  |  |
| 4. | Memorija DRAM 32GB (2X 16GB ) DDR5-5600 UDIMM CL46 | 11 |  |  |  |
| 5. | SSD 1TB M.2 2280 PCIe 4.0 NVMe SSD , EAN: 740617344790,minimun Sequential Read Rate 4900 MB/s, Maximum Sequential Write Rate 4000 MB/s, TBW minimum 600 | 11 |  |  |  |
| 6. | Napajanje 700W PSU 80 PLUS, ATX12V V2.31 | Active PFC | 120mm quiet fan | Flat cables | Single rail power for ATX12V | 1x ATX 24 pin & 20 pin | 1x EPS/ATX12V 8-4 pin | 2x PCI-E 6+2 pin | 3x SATA | 4x 4 pin peripheral | 1x floppy | | 11 |  |  |  |
| 7. | Grafička kartica RTX 4060 Boost Clock (MHz): 2460 | Base Clock(MHz): 1830 | Minimum, dimenzije 250mm x 118mm x 42mm | 11 |  |  |  |
| 8. | Kućište MIDI Tower , dimenzije 400 x 206 x 458 (H)mm | 11 |  |  |  |
| 9. | Monitor 25“ IPS, FHD, 280Hz, HDMI, 2xDP, 1ms | 11 |  |  |  |
| 10. | Tipkovnica bežična ergonomična , Bluetooth, dimenzije 375.97 x 218.91 x 30.53 mm, težina 750g | 11 |  |  |  |
| 11. | Miš bežični, minimum 10000 dpi | 11 |  |  |  |
| 12. | Podloga za miš | 11 |  |  |  |
| UKUPNA CIJENA BEZ PDV-a: |  |
|  IZNOS PDV-a: |  |
| UKUPNA CIJENA S PDV-om: |  |

 U \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, dana \_\_\_\_\_\_\_\_\_\_\_\_2025. godine

 M.P.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(ime, prezime, funkcija i potpis ovlaštene osobe ponuditelja)